

**Practical 03 Configure VLAN and Perform Inter VLAN Routing in Packet Tracer.**


**Step-1: Take Multilayer switch and connect devices to switch as shown below.**

****


**Step-2: Click on Switch -> Go to CLI and enter configuration commands as shown here.**


****

**Step-3: Configure IP address ,subnet mask and default gateway for each device as shown below.**

****

**Step-4: Open Command Prompt -> Apply ping command and the result would be as given below.**

****

****